<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<text>Einschub - Steuerung</text>
<text>12V</text>
<text>SCL</text>
<text>SDA</text>
<text>SCL</text>
<text>SDA</text>
<text>+5V</text>
<text>I2C-BUS</text>
<text>I2C</text>
<text>ES</text>
<hole x="198.12" y="76.2" drill="5.08"/>
<hole x="198.12" y="68.58" drill="5.08"/>
<hole x="198.12" y="60.96" drill="5.08"/>
<hole x="76.2" y="68.58" drill="5.08"/>
<hole x="76.2" y="76.2" drill="5.08"/>
<hole x="198.12" y="127" drill="5.08"/>
<hole x="96.52" y="127" drill="5.08"/>
<hole x="76.2" y="60.96" drill="5.08"/>
<hole x="96.52" y="68.58" drill="5.08"/>
<hole x="96.52" y="60.96" drill="5.08"/>
<hole x="55.88" y="76.2" drill="5.08"/>
<text>+15V</text>
<text>UB</text>
<text>URX</text>
<text>Mute</text>
<text>AGC</text>
<text>GND</text>
<text>SDA</text>
<text>SCL</text>
<text>P/N</text>
<text>Vexp</text>
<text>ULNC</text>
<text>GND</text>
<text>VOSD</text>
<text>VIDEO</text>
<text>AUDIO</text>
<text>VIDEO</text>
<text>AUDIO</text>
<text>VOSD</text>
<hole x="157.48" y="127" drill="5.08"/>
<hole x="157.48" y="76.2" drill="5.08"/>
<hole x="157.48" y="68.58" drill="5.08"/>
<hole x="157.48" y="60.96" drill="5.08"/>
<hole x="116.84" y="76.2" drill="5.08"/>
<hole x="116.84" y="68.58" drill="5.08"/>
<hole x="116.84" y="60.96" drill="5.08"/>
<hole x="116.84" y="127" drill="5.08"/>
<text>UB</text>
<text>15V</text>
<text>SC</text>
<text>SD</text>
<text>SYNC</text>
<text>PCF</text>
<text>GND</text>
<text>GND</text>
<text>VIDEO</text>
<text>AUDIO</text>
<text>VOSD</text>
<text>VIDEO</text>
<text>AUDIO</text>
<text>10</text>
<text>11</text>
<text>12</text>
<text>13</text>
<text>14</text>
<text>15</text>
<text>16</text>
<text>17</text>
<text>18</text>
<text>19</text>
<text>20</text>
<text>21</text>
<text>23</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>8</text>
<text>9</text>
<text>10</text>
<text>11</text>
<text>12</text>
<text>13</text>
<text>14</text>
<text>15</text>
<text>16</text>
<text>17</text>
<text>19</text>
<text>18</text>
<text>20</text>
<text>21</text>
<hole x="96.52" y="77.47" drill="5.08"/>
<hole x="55.88" y="68.58" drill="5.08"/>
<hole x="55.88" y="60.96" drill="5.08"/>
<hole x="-55.5625" y="142.875" drill="2.8"/>
<hole x="5.3975" y="142.875" drill="2.8"/>
<hole x="25.7175" y="142.875" drill="2.8"/>
<hole x="46.0375" y="142.875" drill="2.8"/>
<hole x="66.3575" y="142.875" drill="2.8"/>
<hole x="86.6775" y="142.875" drill="2.8"/>
<hole x="106.9975" y="142.875" drill="2.8"/>
<hole x="167.9575" y="52.705" drill="2.8"/>
<hole x="127.3175" y="52.705" drill="2.8"/>
<hole x="-25.0825" y="52.705" drill="2.8"/>
<hole x="-14.9225" y="52.705" drill="2.8"/>
<hole x="-75.8825" y="52.705" drill="2.8"/>
<hole x="-55.5625" y="52.705" drill="2.8"/>
<hole x="-167.3225" y="52.705" drill="2.8"/>
<text>EST</text>
<text>I2C</text>
<text>RXATV</text>
<text>RXATV</text>
<text>STX</text>
<text>TX1</text>
<text>RX1</text>
<text>RS</text>
<text>DTMF</text>
<text>AFSK</text>
<text>TX2</text>
<text>RX2</text>
<text>VMUX</text>
<text>AMIX</text>
<text>SCL</text>
<text>SDA</text>
<wire x1="210.82" y1="34.925" x2="210.82" y2="161.925" width="0" layer="20"/>
<wire x1="210.82" y1="161.925" x2="-203.2" y2="161.925" width="0" layer="20"/>
<wire x1="-203.2" y1="161.925" x2="-203.2" y2="33.655" width="0" layer="20"/>
<wire x1="-203.2" y1="33.655" x2="210.82" y2="34.925" width="0" layer="20"/>
<text>RX-ST</text>
<wire x1="190.3" y1="36.6" x2="206.9" y2="36.6" width="0" layer="20"/>
<hole x="-202.8825" y="142.875" drill="2.8"/>
<hole x="-197.8025" y="142.875" drill="2.8"/>
<hole x="208.5975" y="142.875" drill="2.8"/>
<hole x="188.2775" y="142.875" drill="2.8"/>
<hole x="208.5975" y="52.705" drill="2.8"/>
<hole x="-202.8825" y="52.705" drill="2.8"/>
<hole x="-197.8025" y="52.705" drill="2.8"/>
<text>RXneu</text>
<text>UB</text>
<text>RES</text>
<text>XB</text>
<text>XC</text>
<text>RX-ST</text>
<text>BB</text>
<hole x="55.88" y="127" drill="5.08"/>
<hole x="35.56" y="76.2" drill="5.08"/>
<hole x="35.56" y="68.58" drill="5.08"/>
<hole x="35.56" y="60.96" drill="5.08"/>
<text>SC</text>
<text>SD</text>
<text>ON</text>
<text>PCF</text>
<text>UB</text>
<text>15V</text>
<text>GND</text>
<text>GND</text>
<text>VIDEO</text>
<text>AUDIO</text>
<text>BB-OUT</text>
<hole x="35.56" y="127" drill="5.08"/>
<text>BB</text>
<text>PLY</text>
<text>FMTRX</text>
<hole x="15.24" y="127" drill="5.08"/>
<hole x="76.2" y="127" drill="5.08"/>
<hole x="15.24" y="60.96" drill="5.08"/>
<hole x="15.24" y="68.58" drill="5.08"/>
<hole x="15.24" y="76.2" drill="5.08"/>
<hole x="-177.4825" y="52.705" drill="2.8"/>
<hole x="-157.1625" y="52.705" drill="2.8"/>
<hole x="-136.8425" y="52.705" drill="2.8"/>
<hole x="-116.5225" y="52.705" drill="2.8"/>
<hole x="-96.2025" y="52.705" drill="2.8"/>
<hole x="-177.4825" y="142.875" drill="2.8"/>
<hole x="-157.1625" y="142.875" drill="2.8"/>
<hole x="-136.8425" y="142.875" drill="2.8"/>
<hole x="-116.5225" y="142.875" drill="2.8"/>
<hole x="-96.2025" y="142.875" drill="2.8"/>
<hole x="-45.4025" y="142.875" drill="2.8"/>
<hole x="-75.8825" y="142.875" drill="2.8"/>
<hole x="127.3175" y="142.875" drill="2.8"/>
<hole x="147.6375" y="142.875" drill="2.8"/>
<hole x="167.9575" y="142.875" drill="2.8"/>
<text>BUS</text>
<text>NTRS</text>
<hole x="-45.4025" y="52.705" drill="2.8"/>
<hole x="-14.9225" y="142.875" drill="2.8"/>
<hole x="-25.0825" y="142.875" drill="2.8"/>
<text>REL</text>
<text>EXT</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>6</text>
<text>SC1</text>
<text>SD1</text>
<text>SY1</text>
<text>PCF</text>
<text>DA</text>
<text>CL</text>
<text>EN</text>
<text>GND</text>
<text>GND</text>
<text>AGC</text>
<text>GND</text>
<text>GND</text>
<text>OSD</text>
<text>V1</text>
<text>A1</text>
<text>OSD</text>
<text>V1</text>
<text>A1</text>
<text>RL1</text>
<text>RL2</text>
<text>RL3</text>
<text>RL4</text>
<text>RL5</text>
<text>RL6</text>
<text>RL7</text>
<text>RL8</text>
<text>RL9</text>
<text>RL10</text>
<text>RL11</text>
<text>RL12</text>
<text>RS</text>
<text>DCF</text>
</plain>
<libraries>
<library name="con-vg">
<description>&lt;b&gt;VG Connectors (DIN 41612/DIN 41617)&lt;/b&gt;&lt;p&gt;
The library contains devices which allow to place the contacts individually or 
in one or several blocks.&lt;p&gt;
This behavior is indicated by the key words &lt;i&gt;single&lt;/i&gt; and &lt;i&gt;block&lt;/i&gt; in
the respective device descriptions.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="FAC64S">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
female, 64 pins, type C, rows AC, grid 5.08 mm</description>
</package>
<package name="F42-6M">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
female, 42 pins + 6 coax, type C</description>
</package>
<package name="FABC96S">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
female, 96 pins, type C, rows ABC, grid 2.54 mm</description>
</package>
</packages>
</library>
<library name="con-lstb">
<description>&lt;b&gt;Pin Headers&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
MA = male&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MA08-2">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="JP1">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-ml">
<description>&lt;b&gt;Harting  Connectors&lt;/b&gt;&lt;p&gt;
Low profile connectors, straight&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="ML40">
<description>&lt;b&gt;HARTING&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-wago-500">
<description>&lt;b&gt;Wago Screw Clamps&lt;/b&gt;&lt;p&gt;
Grid 5.00 mm&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="W237-103">
<description>&lt;b&gt;WAGO SCREW CLAMP&lt;/b&gt;</description>
</package>
<package name="W237-102">
<description>&lt;b&gt;WAGO SCREW CLAMP&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-harting-ml">
<description>&lt;b&gt;Harting  &amp; 3M Connectors&lt;/b&gt;&lt;p&gt;
Low profile connectors, straight&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="ML10">
<description>&lt;b&gt;HARTING&lt;/b&gt;</description>
</package>
<package name="ML16">
<description>&lt;b&gt;HARTING&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-coax">
<description>&lt;b&gt;Coax Connectors&lt;/b&gt;&lt;p&gt;
Radiall  and M/A COM.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B35N61">
<description>&lt;b&gt;BNC CONNECTOR&lt;/b&gt;&lt;p&gt;
M/A COM&lt;p&gt;
www.macom.com&lt;p&gt;
distributor Farnell 149-452</description>
</package>
</packages>
</library>
<library name="con-amp-quick">
<description>&lt;b&gt;AMP Connectors, Type QUICK&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="05P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="AUDIO-EIN" library="con-lstb" package="MA08-2" value="">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="AUDIO-AUS" library="con-lstb" package="MA08-2" value="">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ST1" library="con-vg" package="FAC64S" value="FAC64S">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="I²C-ST" library="con-vg" package="FAC64S" value="FAC64S">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BUS" library="con-vg" package="FAC64S" value="FAC64S">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ES-ST" library="con-vg" package="FAC64S" value="FAC64S">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RX1" library="con-vg" package="F42-6M" value="F42-6M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RX3" library="con-vg" package="F42-6M" value="F42-6M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="V-MUX" library="con-vg" package="FABC96S" value="FABC96S">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RX4" library="con-vg" package="F42-6M" value="F42-6M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TRX" library="con-vg" package="F42-6M" value="F42-6M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ST2" library="con-vg" package="FAC64S" value="FAC64S">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RX2" library="con-vg" package="F42-6M" value="F42-6M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SV1" library="con-ml" package="ML40" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="SV3" library="con-ml" package="ML40" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="PLY" library="con-vg" package="F42-6M" value="F42-6M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PLY1" library="con-vg" package="F42-6M" value="F42-6M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PLY2" library="con-vg" package="F42-6M" value="F42-6M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="con-wago-500" package="W237-103" value="">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="237-103"/>
<attribute name="OC_NEWARK" value="18M7116"/>
</element>
<element name="A-MIX1" library="con-vg" package="FABC96S" value="FABC96S">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X4" library="con-wago-500" package="W237-103" value="">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="237-103"/>
<attribute name="OC_NEWARK" value="18M7116"/>
</element>
<element name="X5" library="con-wago-500" package="W237-102" value="">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="237-102"/>
<attribute name="OC_NEWARK" value="70K9898"/>
</element>
<element name="X6" library="con-wago-500" package="W237-102" value="">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="237-102"/>
<attribute name="OC_NEWARK" value="70K9898"/>
</element>
<element name="JP3" library="jumper" package="JP1" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="jumper" package="JP1" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="jumper" package="JP1" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP6" library="jumper" package="JP1" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP7" library="jumper" package="JP1" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP8" library="jumper" package="JP1" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP9" library="jumper" package="JP1" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP10" library="jumper" package="JP1" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="V1" library="con-coax" package="B35N61" value="BN35N61">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="NAME"/>
</element>
<element name="A1" library="con-coax" package="B35N61" value="BN35N61">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="NAME"/>
</element>
<element name="O1" library="con-coax" package="B35N61" value="BN35N61">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="NAME"/>
</element>
<element name="V2" library="con-coax" package="B35N61" value="BN35N61">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="NAME"/>
</element>
<element name="A2" library="con-coax" package="B35N61" value="BN35N61">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="NAME"/>
</element>
<element name="O2" library="con-coax" package="B35N61" value="BN35N61">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="NAME"/>
</element>
<element name="V5" library="con-coax" package="B35N61" value="BN35N61">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="NAME"/>
</element>
<element name="A5" library="con-coax" package="B35N61" value="BN35N61">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="NAME"/>
</element>
<element name="V6" library="con-coax" package="B35N61" value="BN35N61">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="NAME"/>
</element>
<element name="A6" library="con-coax" package="B35N61" value="BN35N61">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="NAME"/>
</element>
<element name="V7" library="con-coax" package="B35N61" value="BN35N61">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="NAME"/>
</element>
<element name="A7" library="con-coax" package="B35N61" value="BN35N61">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="NAME"/>
</element>
<element name="V8" library="con-coax" package="B35N61" value="BN35N61">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="NAME"/>
</element>
<element name="A8" library="con-coax" package="B35N61" value="BN35N61">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="NAME"/>
</element>
<element name="V3" library="con-coax" package="B35N61" value="BN35N61">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="NAME"/>
</element>
<element name="A3" library="con-coax" package="B35N61" value="BN35N61">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="NAME"/>
</element>
<element name="V4" library="con-coax" package="B35N61" value="BN35N61">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="NAME"/>
</element>
<element name="A4" library="con-coax" package="B35N61" value="BN35N61">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="NAME"/>
</element>
<element name="X2" library="con-wago-500" package="W237-102" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="237-102"/>
<attribute name="OC_NEWARK" value="70K9898"/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="REL" library="con-vg" package="FAC64S" value="FAC64S">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S-R3" library="con-harting-ml" package="ML10" value="">
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="EXT" library="con-vg" package="FAC64S" value="FAC64S">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VIDEO-EIN1" library="con-lstb" package="MA08-2" value="">
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
</element>
<element name="VIDEO-AUS1" library="con-lstb" package="MA08-2" value="">
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
</element>
<element name="SX1" library="con-wago-500" package="W237-102" value="">
<attribute name="OC_NEWARK" value="70K9898"/>
<attribute name="MPN" value="237-102"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="SX2" library="con-wago-500" package="W237-102" value="">
<attribute name="OC_NEWARK" value="70K9898"/>
<attribute name="MPN" value="237-102"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="SX3" library="con-wago-500" package="W237-102" value="">
<attribute name="OC_NEWARK" value="70K9898"/>
<attribute name="MPN" value="237-102"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="SX5" library="con-wago-500" package="W237-102" value="">
<attribute name="OC_NEWARK" value="70K9898"/>
<attribute name="MPN" value="237-102"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="SX6" library="con-wago-500" package="W237-102" value="">
<attribute name="OC_NEWARK" value="70K9898"/>
<attribute name="MPN" value="237-102"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="SX4" library="con-wago-500" package="W237-102" value="">
<attribute name="OC_NEWARK" value="70K9898"/>
<attribute name="MPN" value="237-102"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="SX7" library="con-wago-500" package="W237-102" value="">
<attribute name="OC_NEWARK" value="70K9898"/>
<attribute name="MPN" value="237-102"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="S-PCF" library="con-harting-ml" package="ML10" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RES" library="con-vg" package="FAC64S" value="FAC64S">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S-DAT" library="con-harting-ml" package="ML16" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S-BUS" library="con-amp-quick" package="05P" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S-R2" library="con-harting-ml" package="ML10" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S-R1" library="con-harting-ml" package="ML10" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$7">
</signal>
<signal name="N$8">
</signal>
<signal name="GND">
<contactref element="ST1" pad="A20"/>
<contactref element="ST1" pad="C20"/>
<contactref element="ST1" pad="A14"/>
<contactref element="ST1" pad="C14"/>
<contactref element="ST1" pad="A32"/>
<contactref element="ST1" pad="C32"/>
<contactref element="I²C-ST" pad="A14"/>
<contactref element="I²C-ST" pad="C14"/>
<contactref element="I²C-ST" pad="A20"/>
<contactref element="I²C-ST" pad="C20"/>
<contactref element="BUS" pad="A14"/>
<contactref element="BUS" pad="C14"/>
<contactref element="ES-ST" pad="A14"/>
<contactref element="ES-ST" pad="C14"/>
<contactref element="BUS" pad="A20"/>
<contactref element="BUS" pad="C20"/>
<contactref element="ES-ST" pad="A20"/>
<contactref element="ES-ST" pad="C20"/>
<contactref element="RX1" pad="C14"/>
<contactref element="RX1" pad="C20"/>
<contactref element="RX1" pad="B14"/>
<contactref element="RX1" pad="A14"/>
<contactref element="RX1" pad="B20"/>
<contactref element="RX1" pad="A20"/>
<contactref element="V-MUX" pad="A32"/>
<contactref element="V-MUX" pad="B32"/>
<contactref element="V-MUX" pad="C32"/>
<contactref element="TRX" pad="A20"/>
<contactref element="TRX" pad="B20"/>
<contactref element="TRX" pad="C20"/>
<contactref element="TRX" pad="A14"/>
<contactref element="TRX" pad="B14"/>
<contactref element="TRX" pad="C14"/>
<contactref element="ST2" pad="A20"/>
<contactref element="ST2" pad="C20"/>
<contactref element="ST2" pad="A14"/>
<contactref element="ST2" pad="C14"/>
<contactref element="ST2" pad="A32"/>
<contactref element="ST2" pad="C32"/>
<contactref element="RX2" pad="C14"/>
<contactref element="RX2" pad="B14"/>
<contactref element="RX2" pad="A14"/>
<contactref element="RX2" pad="C20"/>
<contactref element="RX2" pad="B20"/>
<contactref element="RX2" pad="A20"/>
<contactref element="PLY" pad="A20"/>
<contactref element="PLY" pad="B20"/>
<contactref element="PLY" pad="C20"/>
<contactref element="PLY" pad="A14"/>
<contactref element="PLY" pad="B14"/>
<contactref element="PLY" pad="C14"/>
<contactref element="RX3" pad="A14"/>
<contactref element="RX3" pad="B14"/>
<contactref element="RX3" pad="C14"/>
<contactref element="RX3" pad="A20"/>
<contactref element="RX3" pad="B20"/>
<contactref element="RX3" pad="C20"/>
<contactref element="RX4" pad="A14"/>
<contactref element="RX4" pad="B14"/>
<contactref element="RX4" pad="C14"/>
<contactref element="RX4" pad="A20"/>
<contactref element="RX4" pad="B20"/>
<contactref element="RX4" pad="C20"/>
<contactref element="PLY1" pad="A20"/>
<contactref element="PLY1" pad="B20"/>
<contactref element="PLY1" pad="C20"/>
<contactref element="PLY1" pad="A14"/>
<contactref element="PLY1" pad="B14"/>
<contactref element="PLY1" pad="C14"/>
<contactref element="PLY2" pad="A20"/>
<contactref element="PLY2" pad="B20"/>
<contactref element="PLY2" pad="C20"/>
<contactref element="PLY2" pad="A14"/>
<contactref element="PLY2" pad="B14"/>
<contactref element="PLY2" pad="C14"/>
<contactref element="I²C-ST" pad="A32"/>
<contactref element="I²C-ST" pad="C32"/>
<contactref element="X5" pad="1"/>
<contactref element="X5" pad="2"/>
<contactref element="BUS" pad="A32"/>
<contactref element="BUS" pad="C32"/>
<contactref element="V2" pad="5"/>
<contactref element="V2" pad="2"/>
<contactref element="V2" pad="4"/>
<contactref element="V2" pad="3"/>
<contactref element="A2" pad="5"/>
<contactref element="A2" pad="2"/>
<contactref element="A2" pad="4"/>
<contactref element="A2" pad="3"/>
<contactref element="O2" pad="5"/>
<contactref element="O2" pad="2"/>
<contactref element="O2" pad="4"/>
<contactref element="O2" pad="3"/>
<contactref element="V1" pad="5"/>
<contactref element="V1" pad="2"/>
<contactref element="V1" pad="4"/>
<contactref element="V1" pad="3"/>
<contactref element="A1" pad="5"/>
<contactref element="A1" pad="2"/>
<contactref element="A1" pad="4"/>
<contactref element="A1" pad="3"/>
<contactref element="O1" pad="5"/>
<contactref element="O1" pad="2"/>
<contactref element="O1" pad="4"/>
<contactref element="O1" pad="3"/>
<contactref element="V4" pad="5"/>
<contactref element="V4" pad="2"/>
<contactref element="V4" pad="4"/>
<contactref element="V4" pad="3"/>
<contactref element="A4" pad="5"/>
<contactref element="A4" pad="2"/>
<contactref element="A4" pad="4"/>
<contactref element="A4" pad="3"/>
<contactref element="V3" pad="5"/>
<contactref element="V3" pad="2"/>
<contactref element="V3" pad="4"/>
<contactref element="V3" pad="3"/>
<contactref element="A3" pad="5"/>
<contactref element="A3" pad="2"/>
<contactref element="A3" pad="4"/>
<contactref element="A3" pad="3"/>
<contactref element="V8" pad="5"/>
<contactref element="V8" pad="2"/>
<contactref element="V8" pad="4"/>
<contactref element="V8" pad="3"/>
<contactref element="A8" pad="5"/>
<contactref element="A8" pad="2"/>
<contactref element="A8" pad="4"/>
<contactref element="A8" pad="3"/>
<contactref element="V7" pad="5"/>
<contactref element="V7" pad="2"/>
<contactref element="V7" pad="4"/>
<contactref element="V7" pad="3"/>
<contactref element="A7" pad="5"/>
<contactref element="A7" pad="2"/>
<contactref element="A7" pad="4"/>
<contactref element="A7" pad="3"/>
<contactref element="V6" pad="5"/>
<contactref element="V6" pad="2"/>
<contactref element="V6" pad="4"/>
<contactref element="V6" pad="3"/>
<contactref element="A6" pad="5"/>
<contactref element="A6" pad="2"/>
<contactref element="A6" pad="4"/>
<contactref element="A6" pad="3"/>
<contactref element="V5" pad="5"/>
<contactref element="V5" pad="2"/>
<contactref element="V5" pad="4"/>
<contactref element="V5" pad="3"/>
<contactref element="A5" pad="5"/>
<contactref element="A5" pad="2"/>
<contactref element="A5" pad="4"/>
<contactref element="A5" pad="3"/>
<contactref element="A-MIX1" pad="A32"/>
<contactref element="A-MIX1" pad="B32"/>
<contactref element="A-MIX1" pad="C32"/>
<contactref element="ES-ST" pad="A32"/>
<contactref element="ES-ST" pad="C32"/>
<contactref element="X2" pad="2"/>
<contactref element="X2" pad="1"/>
<contactref element="REL" pad="C32"/>
<contactref element="REL" pad="A32"/>
<contactref element="EXT" pad="A32"/>
<contactref element="EXT" pad="C32"/>
<contactref element="EXT" pad="A14"/>
<contactref element="EXT" pad="C14"/>
<contactref element="EXT" pad="A20"/>
<contactref element="EXT" pad="C20"/>
<contactref element="SX3" pad="1"/>
<contactref element="SX4" pad="1"/>
<contactref element="SX6" pad="1"/>
<contactref element="SX5" pad="1"/>
<contactref element="SX7" pad="1"/>
<contactref element="SX1" pad="1"/>
<contactref element="SX2" pad="1"/>
<contactref element="S-PCF" pad="9"/>
<contactref element="S-PCF" pad="10"/>
<contactref element="RES" pad="A32"/>
<contactref element="RES" pad="C32"/>
<contactref element="S-DAT" pad="14"/>
<contactref element="S-DAT" pad="16"/>
<contactref element="S-DAT" pad="8"/>
<contactref element="S-DAT" pad="10"/>
<contactref element="S-BUS" pad="3"/>
<contactref element="S-R2" pad="10"/>
<contactref element="S-R2" pad="9"/>
<contactref element="S-R3" pad="9"/>
<contactref element="S-R3" pad="10"/>
<contactref element="S-R1" pad="10"/>
</signal>
<signal name="SC2">
<contactref element="ES-ST" pad="C10"/>
<contactref element="ST2" pad="C4"/>
<contactref element="SV1" pad="9"/>
<contactref element="SV3" pad="9"/>
<contactref element="JP7" pad="1"/>
</signal>
<signal name="SC1">
<contactref element="ES-ST" pad="C7"/>
<contactref element="ST1" pad="C4"/>
<contactref element="SV1" pad="3"/>
<contactref element="SV3" pad="3"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="SC3">
<contactref element="ES-ST" pad="C13"/>
<contactref element="SV1" pad="15"/>
<contactref element="SV3" pad="15"/>
<contactref element="RX3" pad="C15"/>
</signal>
<signal name="SD2">
<contactref element="ES-ST" pad="C9"/>
<contactref element="ST2" pad="C5"/>
<contactref element="SV1" pad="11"/>
<contactref element="SV3" pad="11"/>
<contactref element="JP8" pad="1"/>
</signal>
<signal name="SD1">
<contactref element="ES-ST" pad="C6"/>
<contactref element="ST1" pad="C5"/>
<contactref element="SV1" pad="5"/>
<contactref element="SV3" pad="5"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="ULNC-2">
<contactref element="ST2" pad="A19"/>
<contactref element="ST2" pad="C19"/>
<contactref element="RX2" pad="A19"/>
<contactref element="RX2" pad="B19"/>
<contactref element="RX2" pad="C19"/>
<contactref element="SX2" pad="2"/>
</signal>
<signal name="ULNC-1">
<contactref element="ST1" pad="A19"/>
<contactref element="ST1" pad="C19"/>
<contactref element="RX1" pad="A19"/>
<contactref element="RX1" pad="B19"/>
<contactref element="RX1" pad="C19"/>
<contactref element="SX1" pad="2"/>
</signal>
<signal name="SC4">
<contactref element="ES-ST" pad="C16"/>
<contactref element="SV1" pad="21"/>
<contactref element="SV3" pad="21"/>
<contactref element="RX4" pad="C15"/>
</signal>
<signal name="SD3">
<contactref element="ES-ST" pad="C12"/>
<contactref element="SV1" pad="17"/>
<contactref element="SV3" pad="17"/>
<contactref element="RX3" pad="C16"/>
</signal>
<signal name="SD4">
<contactref element="ES-ST" pad="C15"/>
<contactref element="SV1" pad="23"/>
<contactref element="SV3" pad="23"/>
<contactref element="RX4" pad="C16"/>
</signal>
<signal name="ON6">
<contactref element="I²C-ST" pad="C11"/>
<contactref element="SV1" pad="18"/>
<contactref element="SV3" pad="18"/>
<contactref element="PLY" pad="C17"/>
</signal>
<signal name="N$38">
</signal>
<signal name="ON7">
<contactref element="I²C-ST" pad="C12"/>
<contactref element="SV1" pad="24"/>
<contactref element="SV3" pad="24"/>
<contactref element="PLY1" pad="C17"/>
</signal>
<signal name="N$57">
</signal>
<signal name="N$95">
</signal>
<signal name="N$557">
</signal>
<signal name="SCL">
<contactref element="I²C-ST" pad="C4"/>
<contactref element="BUS" pad="C4"/>
<contactref element="ES-ST" pad="C4"/>
<contactref element="V-MUX" pad="B4"/>
<contactref element="V-MUX" pad="C4"/>
<contactref element="SV1" pad="2"/>
<contactref element="SV3" pad="2"/>
<contactref element="A-MIX1" pad="C4"/>
<contactref element="REL" pad="C4"/>
<contactref element="EXT" pad="C4"/>
<contactref element="RES" pad="C4"/>
<contactref element="S-BUS" pad="1"/>
</signal>
<signal name="SY1">
<contactref element="I²C-ST" pad="C6"/>
<contactref element="ST1" pad="C6"/>
<contactref element="SV1" pad="7"/>
<contactref element="SV3" pad="7"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="SD5">
<contactref element="ES-ST" pad="C18"/>
<contactref element="SV1" pad="10"/>
<contactref element="SV3" pad="10"/>
<contactref element="TRX" pad="C16"/>
</signal>
<signal name="SC5">
<contactref element="ES-ST" pad="C19"/>
<contactref element="SV1" pad="8"/>
<contactref element="SV3" pad="8"/>
<contactref element="TRX" pad="C15"/>
</signal>
<signal name="SD6">
<contactref element="ES-ST" pad="C21"/>
<contactref element="SV1" pad="16"/>
<contactref element="SV3" pad="16"/>
<contactref element="PLY" pad="C16"/>
</signal>
<signal name="SC6">
<contactref element="ES-ST" pad="C22"/>
<contactref element="SV1" pad="14"/>
<contactref element="SV3" pad="14"/>
<contactref element="PLY" pad="C15"/>
</signal>
<signal name="SD7">
<contactref element="ES-ST" pad="C24"/>
<contactref element="SV1" pad="22"/>
<contactref element="SV3" pad="22"/>
<contactref element="PLY1" pad="C16"/>
</signal>
<signal name="SC7">
<contactref element="ES-ST" pad="C25"/>
<contactref element="SV1" pad="20"/>
<contactref element="SV3" pad="20"/>
<contactref element="PLY1" pad="C15"/>
</signal>
<signal name="SD8">
<contactref element="ES-ST" pad="C27"/>
<contactref element="SV1" pad="28"/>
<contactref element="SV3" pad="28"/>
<contactref element="PLY2" pad="C16"/>
</signal>
<signal name="SC8">
<contactref element="ES-ST" pad="C28"/>
<contactref element="SV1" pad="26"/>
<contactref element="SV3" pad="26"/>
<contactref element="PLY2" pad="C15"/>
</signal>
<signal name="ON5">
<contactref element="I²C-ST" pad="C10"/>
<contactref element="SV1" pad="12"/>
<contactref element="SV3" pad="12"/>
<contactref element="TRX" pad="C17"/>
</signal>
<signal name="ON8">
<contactref element="I²C-ST" pad="C13"/>
<contactref element="SV1" pad="30"/>
<contactref element="SV3" pad="30"/>
<contactref element="PLY2" pad="C17"/>
</signal>
<signal name="N$173">
</signal>
<signal name="N$178">
</signal>
<signal name="N$180">
</signal>
<signal name="N$190">
</signal>
<signal name="N$199">
</signal>
<signal name="N$202">
</signal>
<signal name="N$203">
</signal>
<signal name="N$205">
</signal>
<signal name="N$212">
</signal>
<signal name="N$127">
</signal>
<signal name="N$454">
</signal>
<signal name="N$455">
</signal>
<signal name="N$456">
</signal>
<signal name="N$457">
</signal>
<signal name="N$458">
</signal>
<signal name="N$459">
</signal>
<signal name="N$460">
</signal>
<signal name="N$461">
</signal>
<signal name="N$478">
</signal>
<signal name="NTRS">
<contactref element="I²C-ST" pad="C25"/>
<contactref element="S-DAT" pad="7"/>
</signal>
<signal name="RX2">
<contactref element="I²C-ST" pad="C22"/>
<contactref element="S-DAT" pad="2"/>
</signal>
<signal name="RS">
<contactref element="ST1" pad="C29"/>
<contactref element="I²C-ST" pad="C29"/>
<contactref element="V-MUX" pad="C6"/>
<contactref element="V-MUX" pad="B6"/>
<contactref element="ST2" pad="C29"/>
<contactref element="SV1" pad="4"/>
<contactref element="SV3" pad="4"/>
<contactref element="A-MIX1" pad="C6"/>
<contactref element="BUS" pad="C29"/>
<contactref element="REL" pad="C29"/>
<contactref element="EXT" pad="C29"/>
<contactref element="ES-ST" pad="C29"/>
<contactref element="RES" pad="C29"/>
<contactref element="S-DAT" pad="12"/>
</signal>
<signal name="DTMF">
<contactref element="I²C-ST" pad="C30"/>
<contactref element="S-DAT" pad="13"/>
</signal>
<signal name="AFSK">
<contactref element="I²C-ST" pad="C31"/>
<contactref element="S-DAT" pad="15"/>
</signal>
<signal name="N$527">
</signal>
<signal name="N$151">
</signal>
<signal name="N$153">
</signal>
<signal name="N$367">
</signal>
<signal name="N$370">
</signal>
<signal name="N$387">
</signal>
<signal name="N$389">
</signal>
<signal name="N$390">
</signal>
<signal name="N$422">
</signal>
<signal name="N$425">
</signal>
<signal name="N$154">
</signal>
<signal name="N$155">
</signal>
<signal name="N$156">
</signal>
<signal name="N$157">
</signal>
<signal name="N$158">
</signal>
<signal name="N$400">
</signal>
<signal name="SY3">
<contactref element="I²C-ST" pad="C8"/>
<contactref element="SV1" pad="19"/>
<contactref element="SV3" pad="19"/>
<contactref element="RX3" pad="C17"/>
</signal>
<signal name="SY2">
<contactref element="I²C-ST" pad="C7"/>
<contactref element="ST2" pad="C6"/>
<contactref element="SV1" pad="13"/>
<contactref element="SV3" pad="13"/>
<contactref element="JP9" pad="1"/>
</signal>
<signal name="SY4">
<contactref element="I²C-ST" pad="C9"/>
<contactref element="SV1" pad="25"/>
<contactref element="SV3" pad="25"/>
<contactref element="RX4" pad="C17"/>
</signal>
<signal name="N$290">
</signal>
<signal name="N$408">
</signal>
<signal name="N$553">
</signal>
<signal name="N$554">
</signal>
<signal name="N$555">
</signal>
<signal name="N$601">
</signal>
<signal name="N$444">
</signal>
<signal name="N$445">
</signal>
<signal name="N$446">
</signal>
<signal name="N$69">
</signal>
<signal name="N$89">
</signal>
<signal name="N$90">
</signal>
<signal name="N$91">
</signal>
<signal name="AE1">
<contactref element="AUDIO-EIN" pad="1"/>
</signal>
<signal name="AE2">
<contactref element="AUDIO-EIN" pad="3"/>
</signal>
<signal name="AE3">
<contactref element="AUDIO-EIN" pad="5"/>
</signal>
<signal name="AE4">
<contactref element="AUDIO-EIN" pad="7"/>
</signal>
<signal name="AE5">
<contactref element="AUDIO-EIN" pad="9"/>
</signal>
<signal name="AE6">
<contactref element="AUDIO-EIN" pad="11"/>
</signal>
<signal name="AE7">
<contactref element="AUDIO-EIN" pad="13"/>
</signal>
<signal name="AE8">
<contactref element="AUDIO-EIN" pad="15"/>
</signal>
<signal name="AA8">
<contactref element="AUDIO-AUS" pad="1"/>
</signal>
<signal name="AA7">
<contactref element="AUDIO-AUS" pad="3"/>
</signal>
<signal name="AA6">
<contactref element="AUDIO-AUS" pad="5"/>
</signal>
<signal name="AA5">
<contactref element="AUDIO-AUS" pad="7"/>
</signal>
<signal name="AA1">
<contactref element="AUDIO-AUS" pad="9"/>
</signal>
<signal name="AA2">
<contactref element="AUDIO-AUS" pad="11"/>
</signal>
<signal name="AA3">
<contactref element="AUDIO-AUS" pad="13"/>
</signal>
<signal name="AA4">
<contactref element="AUDIO-AUS" pad="15"/>
</signal>
<signal name="VE1">
<contactref element="VIDEO-EIN1" pad="1"/>
</signal>
<signal name="VE7">
<contactref element="VIDEO-EIN1" pad="13"/>
</signal>
<signal name="VE8">
<contactref element="VIDEO-EIN1" pad="15"/>
</signal>
<signal name="VA8">
<contactref element="VIDEO-AUS1" pad="1"/>
</signal>
<signal name="VA7">
<contactref element="VIDEO-AUS1" pad="3"/>
</signal>
<signal name="VA6">
<contactref element="VIDEO-AUS1" pad="5"/>
</signal>
<signal name="VA5">
<contactref element="VIDEO-AUS1" pad="7"/>
</signal>
<signal name="VA3">
<contactref element="VIDEO-AUS1" pad="13"/>
</signal>
<signal name="VA4">
<contactref element="VIDEO-AUS1" pad="15"/>
</signal>
<signal name="VE6">
<contactref element="VIDEO-EIN1" pad="11"/>
</signal>
<signal name="VE4">
<contactref element="VIDEO-EIN1" pad="7"/>
</signal>
<signal name="VE5">
<contactref element="VIDEO-EIN1" pad="9"/>
</signal>
<signal name="VE3">
<contactref element="VIDEO-EIN1" pad="5"/>
</signal>
<signal name="VE2">
<contactref element="VIDEO-EIN1" pad="3"/>
</signal>
<signal name="VA1">
<contactref element="VIDEO-AUS1" pad="9"/>
</signal>
<signal name="VA2">
<contactref element="VIDEO-AUS1" pad="11"/>
</signal>
<signal name="N$304">
</signal>
<signal name="N$305">
</signal>
<signal name="N$306">
</signal>
<signal name="N$307">
</signal>
<signal name="N$146">
</signal>
<signal name="SDA">
<contactref element="I²C-ST" pad="C5"/>
<contactref element="BUS" pad="C5"/>
<contactref element="ES-ST" pad="C5"/>
<contactref element="V-MUX" pad="C5"/>
<contactref element="V-MUX" pad="B5"/>
<contactref element="SV1" pad="1"/>
<contactref element="SV3" pad="1"/>
<contactref element="A-MIX1" pad="C5"/>
<contactref element="REL" pad="C5"/>
<contactref element="EXT" pad="C5"/>
<contactref element="RES" pad="C5"/>
<contactref element="S-BUS" pad="2"/>
</signal>
<signal name="N$252">
</signal>
<signal name="DA2">
<contactref element="ST2" pad="C15"/>
<contactref element="RX2" pad="C15"/>
<contactref element="JP7" pad="2"/>
</signal>
<signal name="EN2">
<contactref element="ST2" pad="C17"/>
<contactref element="RX2" pad="C17"/>
<contactref element="JP9" pad="2"/>
</signal>
<signal name="CL2">
<contactref element="ST2" pad="C16"/>
<contactref element="RX2" pad="C16"/>
<contactref element="JP8" pad="2"/>
</signal>
<signal name="MUTE2">
<contactref element="ST2" pad="C12"/>
<contactref element="ST2" pad="A12"/>
<contactref element="RX2" pad="A12"/>
<contactref element="RX2" pad="B12"/>
<contactref element="RX2" pad="C12"/>
</signal>
<signal name="N$121">
</signal>
<signal name="N$3">
</signal>
<signal name="N$53">
</signal>
<signal name="N$4">
</signal>
<signal name="N$5">
</signal>
<signal name="RX1">
<contactref element="I²C-ST" pad="C28"/>
<contactref element="S-DAT" pad="11"/>
</signal>
<signal name="TX1">
<contactref element="I²C-ST" pad="C27"/>
<contactref element="S-DAT" pad="9"/>
</signal>
<signal name="N$40">
<contactref element="I²C-ST" pad="C26"/>
</signal>
<signal name="N$42">
<contactref element="I²C-ST" pad="C24"/>
<contactref element="S-DAT" pad="6"/>
</signal>
<signal name="N$75">
</signal>
<signal name="N$81">
</signal>
<signal name="N$118">
<contactref element="ES-ST" pad="C31"/>
</signal>
<signal name="N$119">
<contactref element="ES-ST" pad="C30"/>
</signal>
<signal name="N$129">
</signal>
<signal name="N$132">
</signal>
<signal name="N$138">
</signal>
<signal name="N$145">
</signal>
<signal name="N$147">
</signal>
<signal name="N$149">
</signal>
<signal name="N$150">
</signal>
<signal name="N$161">
</signal>
<signal name="N$163">
</signal>
<signal name="N$243">
</signal>
<signal name="N$245">
</signal>
<signal name="N$246">
</signal>
<signal name="N$247">
</signal>
<signal name="N$263">
</signal>
<signal name="N$278">
</signal>
<signal name="N$282">
</signal>
<signal name="N$283">
</signal>
<signal name="N$284">
</signal>
<signal name="N$288">
</signal>
<signal name="N$289">
</signal>
<signal name="N$291">
</signal>
<signal name="N$293">
</signal>
<signal name="N$294">
</signal>
<signal name="N$323">
</signal>
<signal name="N$329">
</signal>
<signal name="N$332">
</signal>
<signal name="N$334">
</signal>
<signal name="N$335">
</signal>
<signal name="N$336">
</signal>
<signal name="N$343">
</signal>
<signal name="N$344">
</signal>
<signal name="N$345">
</signal>
<signal name="N$354">
</signal>
<signal name="N$356">
</signal>
<signal name="N$357">
</signal>
<signal name="N$359">
</signal>
<signal name="N$360">
</signal>
<signal name="N$361">
</signal>
<signal name="N$365">
</signal>
<signal name="N$373">
</signal>
<signal name="N$375">
</signal>
<signal name="N$376">
</signal>
<signal name="N$377">
</signal>
<signal name="N$382">
</signal>
<signal name="N$384">
</signal>
<signal name="N$388">
</signal>
<signal name="N$392">
</signal>
<signal name="N$398">
</signal>
<signal name="N$401">
</signal>
<signal name="N$402">
</signal>
<signal name="N$411">
</signal>
<signal name="N$412">
</signal>
<signal name="N$413">
</signal>
<signal name="N$416">
</signal>
<signal name="N$420">
</signal>
<signal name="N$427">
</signal>
<signal name="N$428">
</signal>
<signal name="N$429">
</signal>
<signal name="N$430">
</signal>
<signal name="N$433">
</signal>
<signal name="N$434">
</signal>
<signal name="N$435">
</signal>
<signal name="N$436">
</signal>
<signal name="N$437">
</signal>
<signal name="N$438">
</signal>
<signal name="N$441">
</signal>
<signal name="N$442">
</signal>
<signal name="N$443">
</signal>
<signal name="N$447">
</signal>
<signal name="N$449">
</signal>
<signal name="N$450">
</signal>
<signal name="N$451">
</signal>
<signal name="N$453">
</signal>
<signal name="N$462">
</signal>
<signal name="N$463">
</signal>
<signal name="N$466">
</signal>
<signal name="N$467">
</signal>
<signal name="N$468">
</signal>
<signal name="N$471">
</signal>
<signal name="N$473">
</signal>
<signal name="N$477">
</signal>
<signal name="N$484">
</signal>
<signal name="N$486">
</signal>
<signal name="N$487">
</signal>
<signal name="N$495">
</signal>
<signal name="N$496">
</signal>
<signal name="N$498">
</signal>
<signal name="N$499">
</signal>
<signal name="N$500">
</signal>
<signal name="N$502">
</signal>
<signal name="N$504">
</signal>
<signal name="N$505">
</signal>
<signal name="N$506">
</signal>
<signal name="N$507">
</signal>
<signal name="N$508">
</signal>
<signal name="N$510">
</signal>
<signal name="N$512">
</signal>
<signal name="N$514">
</signal>
<signal name="N$515">
</signal>
<signal name="N$516">
</signal>
<signal name="N$518">
</signal>
<signal name="N$520">
</signal>
<signal name="N$521">
</signal>
<signal name="N$522">
</signal>
<signal name="N$529">
</signal>
<signal name="N$530">
</signal>
<signal name="N$531">
</signal>
<signal name="N$532">
</signal>
<signal name="N$533">
</signal>
<signal name="N$536">
</signal>
<signal name="N$537">
</signal>
<signal name="N$538">
</signal>
<signal name="N$539">
</signal>
<signal name="N$543">
</signal>
<signal name="N$545">
</signal>
<signal name="N$546">
</signal>
<signal name="N$547">
</signal>
<signal name="N$550">
</signal>
<signal name="N$556">
</signal>
<signal name="N$560">
</signal>
<signal name="N$561">
</signal>
<signal name="N$562">
</signal>
<signal name="N$566">
</signal>
<signal name="N$569">
</signal>
<signal name="N$570">
</signal>
<signal name="N$575">
</signal>
<signal name="N$578">
</signal>
<signal name="N$579">
</signal>
<signal name="N$580">
</signal>
<signal name="N$591">
</signal>
<signal name="N$595">
</signal>
<signal name="N$596">
</signal>
<signal name="N$597">
</signal>
<signal name="N$598">
</signal>
<signal name="N$605">
</signal>
<signal name="N$606">
</signal>
<signal name="N$614">
</signal>
<signal name="N$615">
</signal>
<signal name="N$617">
</signal>
<signal name="N$618">
</signal>
<signal name="N$620">
</signal>
<signal name="N$621">
</signal>
<signal name="N$622">
</signal>
<signal name="N$631">
</signal>
<signal name="12V4">
<contactref element="RX4" pad="A10"/>
<contactref element="RX4" pad="B10"/>
<contactref element="RX4" pad="C10"/>
</signal>
<signal name="URX4">
<contactref element="RX4" pad="A11"/>
<contactref element="RX4" pad="B11"/>
<contactref element="RX4" pad="C11"/>
</signal>
<signal name="MUTE4">
<contactref element="RX4" pad="A12"/>
<contactref element="RX4" pad="B12"/>
<contactref element="RX4" pad="C12"/>
</signal>
<signal name="AGC1">
<contactref element="ST1" pad="C13"/>
<contactref element="RX1" pad="C13"/>
</signal>
<signal name="DA1">
<contactref element="ST1" pad="C15"/>
<contactref element="RX1" pad="C15"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="CL1">
<contactref element="ST1" pad="C16"/>
<contactref element="RX1" pad="C16"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="VOSD-2">
<contactref element="ST2" pad="C21"/>
<contactref element="RX2" pad="C21"/>
<contactref element="O2" pad="1"/>
</signal>
<signal name="12V2">
<contactref element="ST2" pad="C10"/>
<contactref element="ST2" pad="A10"/>
<contactref element="RX2" pad="A10"/>
<contactref element="RX2" pad="B10"/>
<contactref element="RX2" pad="C10"/>
</signal>
<signal name="12V1">
<contactref element="ST1" pad="A10"/>
<contactref element="ST1" pad="C10"/>
<contactref element="RX1" pad="A10"/>
<contactref element="RX1" pad="B10"/>
<contactref element="RX1" pad="C10"/>
</signal>
<signal name="V1">
<contactref element="ST1" pad="C22"/>
<contactref element="RX1" pad="C22"/>
<contactref element="V1" pad="1"/>
</signal>
<signal name="A1">
<contactref element="ST1" pad="C23"/>
<contactref element="RX1" pad="C23"/>
<contactref element="A1" pad="1"/>
</signal>
<signal name="OSD1">
<contactref element="ST1" pad="C21"/>
<contactref element="RX1" pad="C21"/>
<contactref element="O1" pad="1"/>
</signal>
<signal name="URX1">
<contactref element="ST1" pad="A11"/>
<contactref element="ST1" pad="C11"/>
<contactref element="RX1" pad="A11"/>
<contactref element="RX1" pad="B11"/>
<contactref element="RX1" pad="C11"/>
</signal>
<signal name="MUTE3">
<contactref element="RX3" pad="A12"/>
<contactref element="RX3" pad="B12"/>
<contactref element="RX3" pad="C12"/>
</signal>
<signal name="12V3">
<contactref element="RX3" pad="A10"/>
<contactref element="RX3" pad="B10"/>
<contactref element="RX3" pad="C10"/>
</signal>
<signal name="N$32">
</signal>
<signal name="N$82">
</signal>
<signal name="N$86">
</signal>
<signal name="N$25">
</signal>
<signal name="N$59">
<contactref element="TRX" pad="A19"/>
<contactref element="TRX" pad="B19"/>
<contactref element="TRX" pad="C19"/>
<contactref element="SX5" pad="2"/>
</signal>
<signal name="A6">
<contactref element="PLY" pad="C23"/>
<contactref element="A6" pad="1"/>
</signal>
<signal name="V6">
<contactref element="PLY" pad="C22"/>
<contactref element="V6" pad="1"/>
</signal>
<signal name="N$65">
<contactref element="PLY" pad="C19"/>
<contactref element="PLY" pad="B19"/>
<contactref element="PLY" pad="A19"/>
<contactref element="SX6" pad="2"/>
</signal>
<signal name="V5">
<contactref element="TRX" pad="C22"/>
<contactref element="V5" pad="1"/>
</signal>
<signal name="A5">
<contactref element="TRX" pad="C23"/>
<contactref element="A5" pad="1"/>
</signal>
<signal name="N$68">
</signal>
<signal name="N$72">
</signal>
<signal name="N$92">
</signal>
<signal name="V4">
<contactref element="RX4" pad="C22"/>
<contactref element="V4" pad="1"/>
</signal>
<signal name="A4">
<contactref element="RX4" pad="C23"/>
<contactref element="A4" pad="1"/>
</signal>
<signal name="V3">
<contactref element="RX3" pad="C22"/>
<contactref element="V3" pad="1"/>
</signal>
<signal name="A2">
<contactref element="ST2" pad="C23"/>
<contactref element="RX2" pad="C23"/>
<contactref element="A2" pad="1"/>
</signal>
<signal name="V2">
<contactref element="RX2" pad="C22"/>
<contactref element="ST2" pad="C22"/>
<contactref element="V2" pad="1"/>
</signal>
<signal name="A3">
<contactref element="RX3" pad="C23"/>
<contactref element="A3" pad="1"/>
</signal>
<signal name="V7">
<contactref element="PLY1" pad="C22"/>
<contactref element="V7" pad="1"/>
</signal>
<signal name="A7">
<contactref element="PLY1" pad="C23"/>
<contactref element="A7" pad="1"/>
</signal>
<signal name="A8">
<contactref element="PLY2" pad="C23"/>
<contactref element="A8" pad="1"/>
</signal>
<signal name="V8">
<contactref element="PLY2" pad="C22"/>
<contactref element="V8" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="I²C-ST" pad="A1"/>
<contactref element="I²C-ST" pad="C1"/>
<contactref element="BUS" pad="A1"/>
<contactref element="BUS" pad="C1"/>
<contactref element="ES-ST" pad="A1"/>
<contactref element="ES-ST" pad="C1"/>
<contactref element="A-MIX1" pad="C1"/>
<contactref element="A-MIX1" pad="B1"/>
<contactref element="A-MIX1" pad="A1"/>
<contactref element="X1" pad="3"/>
<contactref element="EXT" pad="A1"/>
<contactref element="EXT" pad="C1"/>
<contactref element="REL" pad="C1"/>
<contactref element="REL" pad="A1"/>
<contactref element="RES" pad="C1"/>
<contactref element="RES" pad="A1"/>
</signal>
<signal name="12V5">
<contactref element="TRX" pad="A10"/>
<contactref element="TRX" pad="B10"/>
<contactref element="TRX" pad="C10"/>
</signal>
<signal name="15V5">
<contactref element="TRX" pad="A12"/>
<contactref element="TRX" pad="B12"/>
<contactref element="TRX" pad="C12"/>
</signal>
<signal name="N$36">
<contactref element="ES-ST" pad="A2"/>
<contactref element="ES-ST" pad="C2"/>
<contactref element="BUS" pad="A2"/>
<contactref element="BUS" pad="C2"/>
<contactref element="I²C-ST" pad="A2"/>
<contactref element="I²C-ST" pad="C2"/>
<contactref element="A-MIX1" pad="B2"/>
<contactref element="A-MIX1" pad="A2"/>
<contactref element="A-MIX1" pad="C2"/>
<contactref element="X1" pad="2"/>
<contactref element="EXT" pad="A2"/>
<contactref element="EXT" pad="C2"/>
<contactref element="REL" pad="C2"/>
<contactref element="REL" pad="A2"/>
<contactref element="RES" pad="C2"/>
<contactref element="RES" pad="A2"/>
</signal>
<signal name="12V6">
<contactref element="PLY" pad="A10"/>
<contactref element="PLY" pad="B10"/>
<contactref element="PLY" pad="C10"/>
</signal>
<signal name="URX6">
<contactref element="PLY" pad="A11"/>
<contactref element="PLY" pad="B11"/>
<contactref element="PLY" pad="C11"/>
</signal>
<signal name="15V6">
<contactref element="PLY" pad="A12"/>
<contactref element="PLY" pad="B12"/>
<contactref element="PLY" pad="C12"/>
</signal>
<signal name="12V7">
<contactref element="PLY1" pad="A10"/>
<contactref element="PLY1" pad="B10"/>
<contactref element="PLY1" pad="C10"/>
</signal>
<signal name="15V7">
<contactref element="PLY1" pad="A12"/>
<contactref element="PLY1" pad="B12"/>
<contactref element="PLY1" pad="C12"/>
</signal>
<signal name="12V8">
<contactref element="PLY2" pad="A10"/>
<contactref element="PLY2" pad="B10"/>
<contactref element="PLY2" pad="C10"/>
</signal>
<signal name="URX8">
<contactref element="PLY2" pad="A11"/>
<contactref element="PLY2" pad="B11"/>
<contactref element="PLY2" pad="C11"/>
</signal>
<signal name="15V8">
<contactref element="PLY2" pad="A12"/>
<contactref element="PLY2" pad="B12"/>
<contactref element="PLY2" pad="C12"/>
</signal>
<signal name="N$64">
<contactref element="ST1" pad="A1"/>
<contactref element="ST1" pad="C1"/>
<contactref element="ST2" pad="A1"/>
<contactref element="ST2" pad="C1"/>
<contactref element="X6" pad="2"/>
<contactref element="V-MUX" pad="A1"/>
<contactref element="V-MUX" pad="C1"/>
<contactref element="X4" pad="1"/>
<contactref element="V-MUX" pad="B1"/>
</signal>
<signal name="N$66">
<contactref element="ST1" pad="A2"/>
<contactref element="ST1" pad="C2"/>
<contactref element="ST2" pad="A2"/>
<contactref element="ST2" pad="C2"/>
<contactref element="V-MUX" pad="A2"/>
<contactref element="V-MUX" pad="C2"/>
<contactref element="X4" pad="2"/>
<contactref element="V-MUX" pad="B2"/>
</signal>
<signal name="N$70">
</signal>
<signal name="N$71">
</signal>
<signal name="N$73">
</signal>
<signal name="N$28">
<contactref element="ST1" pad="A3"/>
<contactref element="ST1" pad="C3"/>
<contactref element="ST2" pad="A3"/>
<contactref element="ST2" pad="C3"/>
<contactref element="X6" pad="1"/>
<contactref element="V-MUX" pad="A3"/>
<contactref element="V-MUX" pad="C3"/>
<contactref element="X4" pad="3"/>
<contactref element="V-MUX" pad="B3"/>
</signal>
<signal name="N$10">
<contactref element="I²C-ST" pad="A3"/>
<contactref element="I²C-ST" pad="C3"/>
<contactref element="BUS" pad="A3"/>
<contactref element="BUS" pad="C3"/>
<contactref element="ES-ST" pad="A3"/>
<contactref element="ES-ST" pad="C3"/>
<contactref element="A-MIX1" pad="B3"/>
<contactref element="A-MIX1" pad="A3"/>
<contactref element="A-MIX1" pad="C3"/>
<contactref element="X1" pad="1"/>
<contactref element="EXT" pad="A3"/>
<contactref element="EXT" pad="C3"/>
<contactref element="REL" pad="C3"/>
<contactref element="REL" pad="A3"/>
<contactref element="RES" pad="A3"/>
<contactref element="RES" pad="C3"/>
</signal>
<signal name="N$6">
<contactref element="PLY1" pad="A19"/>
<contactref element="PLY1" pad="B19"/>
<contactref element="PLY1" pad="C19"/>
<contactref element="SX7" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="PLY2" pad="A19"/>
<contactref element="PLY2" pad="B19"/>
<contactref element="PLY2" pad="C19"/>
</signal>
<signal name="N$13">
<contactref element="RX3" pad="A19"/>
<contactref element="RX3" pad="B19"/>
<contactref element="RX3" pad="C19"/>
<contactref element="SX3" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="RX4" pad="A19"/>
<contactref element="RX4" pad="B19"/>
<contactref element="RX4" pad="C19"/>
<contactref element="SX4" pad="2"/>
</signal>
<signal name="AGC2">
<contactref element="ST2" pad="C13"/>
<contactref element="RX2" pad="C13"/>
</signal>
<signal name="N$54">
<contactref element="REL" pad="C14"/>
<contactref element="S-R2" pad="3"/>
</signal>
<signal name="N$56">
<contactref element="REL" pad="C16"/>
<contactref element="S-R2" pad="5"/>
</signal>
<signal name="N$61">
<contactref element="S-R2" pad="7"/>
<contactref element="REL" pad="C18"/>
</signal>
<signal name="N$63">
<contactref element="REL" pad="C20"/>
<contactref element="S-R3" pad="1"/>
</signal>
<signal name="N$74">
<contactref element="REL" pad="C22"/>
<contactref element="S-R3" pad="3"/>
</signal>
<signal name="N$77">
<contactref element="REL" pad="C24"/>
<contactref element="S-R3" pad="5"/>
</signal>
<signal name="N$79">
<contactref element="REL" pad="C26"/>
<contactref element="S-R3" pad="7"/>
</signal>
<signal name="DCF">
<contactref element="REL" pad="C28"/>
</signal>
<signal name="A">
<contactref element="REL" pad="C8"/>
<contactref element="S-R1" pad="1"/>
</signal>
<signal name="B">
<contactref element="REL" pad="C9"/>
<contactref element="S-R1" pad="3"/>
</signal>
<signal name="C">
<contactref element="REL" pad="C10"/>
<contactref element="S-R1" pad="5"/>
</signal>
<signal name="D">
<contactref element="REL" pad="C11"/>
<contactref element="S-R1" pad="7"/>
</signal>
<signal name="N$55">
<contactref element="REL" pad="C13"/>
<contactref element="S-R2" pad="2"/>
</signal>
<signal name="N$60">
<contactref element="REL" pad="C15"/>
<contactref element="S-R2" pad="4"/>
</signal>
<signal name="N$62">
<contactref element="REL" pad="C17"/>
<contactref element="S-R2" pad="6"/>
</signal>
<signal name="N$67">
<contactref element="REL" pad="C19"/>
<contactref element="S-R2" pad="8"/>
</signal>
<signal name="N$76">
<contactref element="REL" pad="C23"/>
<contactref element="S-R3" pad="4"/>
</signal>
<signal name="N$78">
<contactref element="REL" pad="C25"/>
<contactref element="S-R3" pad="6"/>
</signal>
<signal name="N$80">
<contactref element="REL" pad="C27"/>
<contactref element="S-R3" pad="8"/>
</signal>
<signal name="N$83">
<contactref element="REL" pad="C21"/>
<contactref element="S-R3" pad="2"/>
</signal>
<signal name="PCF1">
<contactref element="BUS" pad="C10"/>
<contactref element="SV1" pad="40"/>
<contactref element="SV3" pad="40"/>
<contactref element="RX1" pad="C18"/>
<contactref element="JP6" pad="2"/>
<contactref element="ST1" pad="C8"/>
<contactref element="JP6" pad="1"/>
<contactref element="S-PCF" pad="1"/>
</signal>
<signal name="PCF2">
<contactref element="BUS" pad="C11"/>
<contactref element="SV1" pad="39"/>
<contactref element="SV3" pad="39"/>
<contactref element="RX2" pad="C18"/>
<contactref element="JP10" pad="2"/>
<contactref element="ST2" pad="C8"/>
<contactref element="JP10" pad="1"/>
<contactref element="S-PCF" pad="2"/>
</signal>
<signal name="PCF3">
<contactref element="BUS" pad="C12"/>
<contactref element="RX3" pad="C18"/>
<contactref element="SV1" pad="37"/>
<contactref element="SV3" pad="37"/>
<contactref element="S-PCF" pad="3"/>
</signal>
<signal name="PCF4">
<contactref element="BUS" pad="C13"/>
<contactref element="RX4" pad="C18"/>
<contactref element="SV1" pad="35"/>
<contactref element="SV3" pad="35"/>
<contactref element="S-PCF" pad="4"/>
</signal>
<signal name="PCF5">
<contactref element="BUS" pad="C15"/>
<contactref element="TRX" pad="C18"/>
<contactref element="SV1" pad="27"/>
<contactref element="SV3" pad="27"/>
<contactref element="S-PCF" pad="5"/>
</signal>
<signal name="PCF6">
<contactref element="BUS" pad="C16"/>
<contactref element="PLY" pad="C18"/>
<contactref element="SV1" pad="29"/>
<contactref element="SV3" pad="29"/>
<contactref element="S-PCF" pad="6"/>
</signal>
<signal name="PCF7">
<contactref element="BUS" pad="C17"/>
<contactref element="PLY1" pad="C18"/>
<contactref element="SV1" pad="31"/>
<contactref element="SV3" pad="31"/>
<contactref element="S-PCF" pad="7"/>
</signal>
<signal name="PCF8">
<contactref element="BUS" pad="C18"/>
<contactref element="PLY2" pad="C18"/>
<contactref element="SV1" pad="33"/>
<contactref element="SV3" pad="33"/>
<contactref element="S-PCF" pad="8"/>
</signal>
<signal name="EN1">
<contactref element="ST1" pad="C17"/>
<contactref element="JP5" pad="2"/>
<contactref element="RX1" pad="C17"/>
</signal>
<signal name="N$1">
<contactref element="AUDIO-EIN" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="AUDIO-EIN" pad="4"/>
</signal>
<signal name="N$9">
<contactref element="AUDIO-EIN" pad="6"/>
</signal>
<signal name="N$11">
<contactref element="AUDIO-EIN" pad="8"/>
</signal>
<signal name="N$15">
<contactref element="AUDIO-EIN" pad="10"/>
</signal>
<signal name="N$16">
<contactref element="AUDIO-EIN" pad="12"/>
</signal>
<signal name="N$17">
<contactref element="AUDIO-EIN" pad="14"/>
</signal>
<signal name="N$18">
<contactref element="AUDIO-EIN" pad="16"/>
</signal>
<signal name="N$19">
<contactref element="AUDIO-AUS" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="AUDIO-AUS" pad="4"/>
</signal>
<signal name="N$21">
<contactref element="AUDIO-AUS" pad="6"/>
</signal>
<signal name="N$22">
<contactref element="AUDIO-AUS" pad="8"/>
</signal>
<signal name="N$23">
<contactref element="AUDIO-AUS" pad="10"/>
</signal>
<signal name="N$24">
<contactref element="AUDIO-AUS" pad="12"/>
</signal>
<signal name="N$26">
<contactref element="AUDIO-AUS" pad="14"/>
</signal>
<signal name="N$27">
<contactref element="AUDIO-AUS" pad="16"/>
</signal>
<signal name="N$30">
<contactref element="A-MIX1" pad="A26"/>
</signal>
<signal name="N$31">
<contactref element="A-MIX1" pad="A27"/>
</signal>
<signal name="N$33">
<contactref element="A-MIX1" pad="A28"/>
</signal>
<signal name="N$34">
<contactref element="A-MIX1" pad="A29"/>
</signal>
<signal name="N$37">
<contactref element="A-MIX1" pad="A30"/>
</signal>
<signal name="N$39">
<contactref element="A-MIX1" pad="A25"/>
</signal>
<signal name="N$41">
<contactref element="A-MIX1" pad="A24"/>
</signal>
<signal name="N$43">
<contactref element="A-MIX1" pad="A31"/>
</signal>
<signal name="N$45">
<contactref element="A-MIX1" pad="A19"/>
</signal>
<signal name="N$46">
<contactref element="A-MIX1" pad="A18"/>
</signal>
<signal name="N$47">
<contactref element="A-MIX1" pad="A17"/>
</signal>
<signal name="N$48">
<contactref element="A-MIX1" pad="A16"/>
</signal>
<signal name="N$49">
<contactref element="A-MIX1" pad="A15"/>
</signal>
<signal name="N$50">
<contactref element="A-MIX1" pad="A14"/>
</signal>
<signal name="N$51">
<contactref element="A-MIX1" pad="A13"/>
</signal>
<signal name="N$52">
<contactref element="A-MIX1" pad="A12"/>
</signal>
<signal name="URX7">
<contactref element="PLY1" pad="A11"/>
<contactref element="PLY1" pad="B11"/>
<contactref element="PLY1" pad="C11"/>
</signal>
<signal name="URX5">
<contactref element="TRX" pad="A11"/>
<contactref element="TRX" pad="B11"/>
<contactref element="TRX" pad="C11"/>
</signal>
<signal name="URX3">
<contactref element="RX3" pad="B11"/>
<contactref element="RX3" pad="C11"/>
<contactref element="RX3" pad="A11"/>
</signal>
<signal name="URX2">
<contactref element="RX2" pad="C11"/>
<contactref element="RX2" pad="B11"/>
<contactref element="RX2" pad="A11"/>
<contactref element="ST2" pad="A11"/>
<contactref element="ST2" pad="C11"/>
</signal>
<signal name="TX2">
<contactref element="I²C-ST" pad="C21"/>
<contactref element="S-DAT" pad="1"/>
</signal>
<signal name="N$44">
<contactref element="I²C-ST" pad="C23"/>
<contactref element="S-DAT" pad="3"/>
</signal>
<signal name="N$84">
<contactref element="ST1" pad="C12"/>
<contactref element="ST1" pad="A12"/>
<contactref element="RX1" pad="C12"/>
<contactref element="RX1" pad="B12"/>
<contactref element="RX1" pad="A12"/>
</signal>
<signal name="N$58">
<contactref element="REL" pad="C12"/>
<contactref element="S-R2" pad="1"/>
</signal>
<signal name="N$85">
<contactref element="S-R1" pad="8"/>
<contactref element="S-R1" pad="2"/>
<contactref element="S-R1" pad="4"/>
<contactref element="S-R1" pad="6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
